**Guide 1**: base (correct) part

1. Base
2. From 1-Base: Positions of Isometric view, View A-A, Section B-B, and Detail C have been moved. Dimensions within those views have not been moved in reference to the views. This is copying.
3. From 1-Base: positions of the dimension numbers have all been moved VERY SLIGHTLY, but none of the view positions have been moved. This is still to be considered copying.
4. From 1-Base: All centerlines and cross-hairs have been removed. No alterations on views placement or dimension number locations. This is copying.
5. All views have been repositioned slightly, some dimensions have been moved slightly, a few missing centerlines. This is an example of a submission with maximum effort not to get caught copying, but should still be considered copying.

**Guide 2**: part file was modified to have longer base (120) and each slot moved 10mm way from center.

2-1 to 2-5: identical to 1-1 to 1-5 but using new modified part. No dimensions were corrected or changed (and thus many are dangling or wrong.)

**Guide 3**: Guide 1 part file was modified so that top row of side holes is below the second row (common error in drawings of this part).

3-1 to 3-5: identical to 1-1 to 1-5 but using new modified part. No dimensions were corrected or changed (and thus many are dangling or wrong.)